

Monitor

API Reference

© 2018 All rights reserved by Metrological

This document contains information which is proprietary and confidential to Metrological. It is provided with the expressed understanding that the recipient will not divulge its content to other parties or otherwise misappropriate the information contained herein. This information is furnished for guidance; specifications and availability of goods mentioned in it are subject to change without notice. No part of this publication may be reproduced, stored in a database, retrieval system or transmitted, in any form or by any means, electronic, mechanical, photocopying, recording or otherwise, without the written prior permission of Metrological.

History

|  |  |  |  |
| --- | --- | --- | --- |
| **Version** | **Date** | **Author** | **Description** |
| 0.1 | 07-01-2017 | C.Custers | Initial version. |
| 0.2 | 12-10-2018 | C.Custers | Move configuration WPEFramework.docx |

Table of Contents

[1. Introduction 4](#__RefHeading___Toc3442_2680829492)

[1.1 Scope 4](#__RefHeading___Toc9782_1911629055)

[1.2 Case sensitivity 4](#__RefHeading___Toc9784_1911629055)

[1.3 Acronyms, Abbreviations and Terms 4](#__RefHeading___Toc9786_1911629055)

[1.4 Standards 4](#__RefHeading___Toc9788_1911629055)

[1.5 References 5](#__RefHeading___Toc9790_1911629055)

[1.6 Open Issues 5](#__RefHeading___Toc9792_1911629055)

[1.7 Limitations 5](#__RefHeading___Toc9794_1911629055)

[2. Monitor Plugin 6](#__RefHeading___Toc3456_2680829492)

[2.1 Configuration of Monitor 6](#__RefHeading___Toc3458_2680829492)

[2.2 Application Programming Interface (API) 6](#__RefHeading___Toc3460_2680829492)

[2.2.1 General information 6](#__RefHeading___Toc3462_2680829492)

[2.2.2 Resetting the statistics 6](#__RefHeading___Toc3464_2680829492)

[2.3 Events 6](#__RefHeading___Toc6089_3082868393)

[2.4 JSON definitions 7](#__RefHeading___Toc6091_3082868393)

[2.4.1 General information 7](#__RefHeading___Toc3462_26808294922)

# Introduction

## Scope

This document describes the Plugin Monitor API interface. This plugin can be configured to be loaded and executed in the WPEFramework and offers user input functionality on the platform. For details on the WPEFramework API, refer to: [[WPEF]](https://github.com/WebPlatformForEmbedded/WPEFramework/blob/master/doc/WPE - API - WPEFramework.docx).

## Case sensitivity

All identifiers on the interface described here are case-sensitive. e.g. an id known in the plugin as 'C0FFEE' is not the same as 'c0ffee'.

All keywords, entities, properties, relations and actions should be treated as case-sensitive.

## Acronyms, Abbreviations and Terms

The next list provides an overview of acronyms and abbreviations used in this document and their definitions.

|  |  |
| --- | --- |
| **Acronym** | **Definitions** |
| API | Application Programming Interface |
| JSON | JavaScript Object Notation |
| UTC | Coordinated Universal Time |

Below terms are listed with their definitions, as used in this document.

|  |  |
| --- | --- |
| **Term** | **Definitions** |
| Callsign | The callsign is the name given to an instance of a plugin. One plugin can be instantiated multiple times, but each instance the instance name, callsign, must be unique. |
| Proxy | An object in one process space representing the “real” object in another process space. The Proxy takes care of marshalling the parameters. |
| Stub | An object in the process space that contains the actual object. The stub takes care of un-marshalling the request from the Proxy and executes the call, on behave of the Proxy object, on the real object |

## Standards

Date time formats between the systems shall be in UTC time and W3C ([[ISO-8601]](http://www.iso.org/iso/date_and_time_format) profile) formatting [[ISO-8601]](http://www.iso.org/iso/date_and_time_format), e.g.: 2004-11-05T13:15:30Z. This way time discontinuities can be avoided due to daylight savings. Note that all interfacing systems must decode/encode the date time to the correct local time.

Languages used in the WPEFramework will be conform [[ISO-639-2]](http://www.loc.gov/standards/iso639-2/php/code_list.php) using two letter language codes. If WPEFramework encounters a language code it does not recognize, it will use ‘xx’ instead. For a list of available two letter ISO language codes, please visit: [[ISO-639-2]](http://www.loc.gov/standards/iso639-2/php/code_list.php).

## References

|  |  |
| --- | --- |
| [[WPEF]](https://github.com/WebPlatformForEmbedded/WPEFramework/blob/master/doc/WPE - API - WPEFramework.docx) | WPEFramework API Reference |
| [[HTTP]](http://www.w3.org/Protocols) | Hypertext Transfer Protocol |
| [[ISO-8601]](http://www.iso.org/iso/date_and_time_format) | Date and time format |
| [[ISO-3166]](http://www.iso.org/iso/country_codes.htm) | Country code specification |
| [[ISO-639-2]](http://www.loc.gov/standards/iso639-2/php/code_list.php) | Language code specification (Alpha-2 code) |
| [[JSON]](http://www.json.org/) | JavaScript Object Notation |
| [[URLENC]](http://www.w3schools.com/tags/ref_urlencode.asp) | URL Encoding |

## Open Issues

This is a list of open issues that needs to be resolved:

* This document is still a work in progress.

## Limitations

The information described in this document is preliminary and subject to change in the future.

Legend:



**Be aware of:** implementation choice is needed or side-effect needs to be handled.



**Implementation advice:** Guide line for implementation mostly related to performance.

# Monitor Plugin

## Configuration of Monitor

See section *Monitor Configuration* of [[WPEF]](https://github.com/WebPlatformForEmbedded/WPEFramework/blob/master/doc/WPE - API - WPEFramework.docx).

## Application Programming Interface (API)

### General information

Using this method, all monitored objects can be retrieved and the associated information.

|  |  |
| --- | --- |
| Request: | GET /Service/Monitor |
| Success: | HTTP/1.1 200 List of monitored plugins  { observer\_list } |
| Failure |  |

|  |  |
| --- | --- |
| Request: | GET /Service/Monitor/<callsign> |
| Success: | HTTP/1.1 200 Monitored plugin statistics  { measurement } |
| Failure | HTTP/1.1 400 Bad request |

### Resetting the statistics

|  |  |
| --- | --- |
| Request: | PUT /Service/Monitor/<callsign> |
| Success: | HTTP/1.1 200 OK  { measurement } |
| Failure | HTTP/1.1 400 Bad request |

All collected information is cleared. The response contains the information just prior to the clear.

## Events

Whenever a plugin that is monitored is deactivated due to an in-operable state or due to exceeding memory usage, it is notified via an event. Also if the monitor is configures to activate a failing plugin, which it monitors, send out an activation event.

|  |  |
| --- | --- |
| callsign | [string] callsign of the plugin applicable for this event. |
| action | [enum] [“Activate”, “Deactivate”] |
| reason | [enum] activate: [“Automatic”]  deactivate: [“MemoryExceeded”, “Failure”] |

## JSON definitions

### General information

All memory measurement are in bytes.

observer\_list:

|  |  |
| --- | --- |
| - | [array] JSON array which consists of observe\_item elements. |

observe\_item:

|  |  |
| --- | --- |
| name | [string] callsign of the plugin being observed. |
| measurement | [JSON] metadata on memory consumption and operational state of the plugin. |

measurement:

|  |  |
| --- | --- |
| allocated {info} | [JSON] virtual memory information as gathered during the last measurement. |
| resident {info} | [JSON] RSS memory information as gathered during the last measurement. |
| shared {info} | [JSON] shared memory information as gathered during the last measurement. |
| process {info} | [JSON] processes allocated to the observed plugin |
| operational | [bool] Was the plugin operational during the last measurement. |
| count | [uint32] number of measurements taken since the plugin is monitored. |

info:

|  |  |
| --- | --- |
| min | [uint64] lowest number measured since the plugin is monitored. |
| max | [uint64] highest number measured since the plugin is monitored. |
| average | [uint64] average number measured since the plugin is monitored. |
| last | [uint64] number measured during the last measurement. |

## 